User shows

Camera

User

Hand gesture

Capture input sign

Image

Output Text

Captured image compared with train & test data

SVM model

Load model

Binary image in

Gray-scale

Image

Input RGB to HSV color image

Extract hand gesture

Detect and track hand

Architecture diagram – Sign Language Recognition